|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | 1A  1 | 2A  2 | 3A  3 | | 4A  4 | 5A  5 | 6A  6 | | 7A  7 | 8A  8 | 9A  9 | | 10A  10 | 11A  11 | 12A  12 |   **Knotted bracelet**: You need 2.6 meters 4 mm Knot line and 1 side release buckle   |  |  | | --- | --- | | MODEL | * Put the middle of the cord through the lock end. Photo 1. * Bring the ends through the loop. Photo 2. * Put the cord through the other lock end. Measure the desired length. Photo 3 * Turn the right cord over the tight center line and place it under the left. Photo 4 * Place left cord under the center line and draw up through the loop and tighten the knot. Photo 5 +6. * Repeat. Start alternately from the right and left. Photo 7 +8 * Finish by cutting the cord about 3 mm and heat seal with a lighter.   Photo 9 +10 +11 (Heat sealing is for Polyester cord only)   * Heat seal string together if knotting with 2 colors. Photo 12 | |