|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |  |
| --- | --- | --- |
| 1A1 | 2A2 | 3A3 |
| 4A4 | 5A5 | 6A6 |
| 7A7 | 8A8 | 9A9 |
| 10A10 | 11A11 | 12A12 |

**Knotted bracelet**: You need 2.6 meters 4 mm Knot line and 1 side release buckle

|  |  |
| --- | --- |
| MODEL | * Put the middle of the cord through the lock end. Photo 1.
* Bring the ends through the loop. Photo 2.
* Put the cord through the other lock end. Measure the desired length. Photo 3
* Turn the right cord over the tight center line and place it under the left. Photo 4
* Place left cord under the center line and draw up through the loop and tighten the knot. Photo 5 +6.
* Repeat. Start alternately from the right and left. Photo 7 +8
* Finish by cutting the cord about 3 mm and heat seal with a lighter.

Photo 9 +10 +11 (Heat sealing is for Polyester cord only)* Heat seal string together if knotting with 2 colors. Photo 12
 |

 |